

**TTL**



****

While sending a PDU,



PC0:





Router0:





Router2:



Router1:





PC1:





While sending response back,



Router1:



Router2:



Router0:



PC0:

